**BOK Systems: BOKHD25G40 Heavy Duty Sub Floor System**

A cradle and batten substructure, comprising of 20mm base and 25mm leg height PU binder and Styrene-Butadiene Rubber shred cradles, 40mm x 40mm BOK-BAT heavy duty battens, 20mm x 150mm foam perimeter flanking strips and a 25mm Tongue & Groove GPT Board 1200mm x 600mm x 25mm.

The installation should be carried out in accordance with BS8203-2001 and installers should refer to the installation drawing, Subfloor to be smooth, hard, clean and dry prior to laying, where applicable the subfloor must incorporate a Damp Proof Membrane.

**Flooring:** Cradle & Batten Undercarriage System

**Supplier and Reference:** Sport & Fitness Flooring Ltd, Wyastone Business Park, Wyastone Leys, Monmouth. NP25 3SR Tel 01600 887521, Email: info@sportandfitnessflooring.com

**Reference:** BOK HD25G40 Heavy Duty System .

**BS EN 685:** Class N/A.

**Finished Floor Height**: 85-124mm

Consult with Sport & Fitness Flooring Ltd for any further requirements and for installation instructions.